VERSION:3 SOURCE_TIMESTAMP:4A3CB0C8
NODE:I LEVEL:0 LINE:24 "C:\Program Files\cvavreal\inc\mega8.h"
NODE:I LEVEL:0 LINE:25 "C:\Program Files\cvavreal\inc\delay.h"
NODE:M LEVEL:0 LINE:27 "ADC_VREF_TYPE"
NODE:M LEVEL:0 LINE:30 "source_but"
NODE:M LEVEL:0 LINE:31 "ch_up_but"
NODE:M LEVEL:0 LINE:32 "ch_down_but"
NODE:M LEVEL:0 LINE:33 "vol_up_but"
NODE:M LEVEL:0 LINE:34 "vol_down_but"
NODE:M LEVEL:0 LINE:35 "speech_but"
NODE:M LEVEL:0 LINE:36 "off_hook_but"
NODE:M LEVEL:0 LINE:37 "on_hook_but"
NODE:V LEVEL:0 LINE:39 "b -> R5"
NODE:V LEVEL:0 LINE:40 "k -> R4"
NODE:V LEVEL:0 LINE:41 "s -> R7"
NODE:F LEVEL:0 LINE:44 "read_adc(unsigned char adc_input)"
NODE:F LEVEL:0 LINE:57 "KEYPRESS(void)"
NODE:F LEVEL:0 LINE:73 "Pressing_long(void)"
NODE:F LEVEL:0 LINE:134 "Pressing_short(void)"
NODE:F LEVEL:0 LINE:192 "All_to_Z(void)"
NODE:F LEVEL:0 LINE:199 "main(void)"
